**FOR IMMEDIATE RELEASE**

**Public Relations Contacts:**

**Amanda Storer, Director Brand Marketing**

Metl-Span

1720 Lakepointe Dr. Ste 101

Lewisville, TX 75057

(972) 221-6656

[AJStorer@metlspan.com](mailto:AJStorer@metlspan.com)

**Jeff Donaldson**

BLD Marketing

(412) 347-8039

[jeff.donaldson@bld-marketing.com](mailto:jeff.donaldson@bld-marketing.com)

**Photos:** <http://www.bldpressroom.com/metl-span/cleanseam>

**Metl-Span introduces FRP CleanSeam™ insulated metal wall panel**

LEWISVILLE, Texas, April 22, 2020 – The new FRP (fiberglass-reinforced plastic) CleanSeam insulated metal wall panel from Metl-Span is designed to provide the appearance of a virtually seamless joint between interior wall panels to prevent water intrusion and bacterial growth. FRP CleanSeam is a perfect solution for commissaries, processing rooms, clean rooms and pharmaceutical manufacturing facilities where frequent wash downs may occur. The reduced-maintenance seal system creates a durable bond – unlike silicone sealants – which can deteriorate under frequent cleanings. FRP is factory-applied, saving labor in the field and offering a durable, corrosion-resistant surface. CleanSeam panels are available in widths of 42 and 44.4 inches, in thicknesses of 2, 3, 4, 5 and 6 inches and anywhere from 8 to 20 feet in length. FRP CleanSeam is available with optional PVC trims for a smooth wall-to-floor or wall-to-ceiling transition.

*Metl-Span is part of the Cornerstone Building Brands family (NYSE: CNR); delivering high-quality, durable and energy-efficient insulated metal panels designed for unparalleled performance to stand the test of time. For more information on Metl-Span products, call 877-585-9969 or visit* [*www.metlspan.com*](http://www.metlspan.com)*.*

# # #